[Table]
ColWidth=640000004B0000004B0000004B0000004B000000640000004B0000004B0000004B000000640000004B0000004B0000004B0000004B0000004B000000640000004B0000004B000000640000004B0000004B000000640000004B0000004B000000
[Chip]
Name=ATmega8515
[CPU]
Clock Frequency=27000000
[Text reports]
Generate lst-file=0
Generate asm-file=1
[Monitor chip]
Using pin=0
[Template]
K_to_Z_Interpretation=1
[Fuse bits]
CKSEL0=1
CKSEL1=1
CKSEL2=1
CKSEL3=1
SUT0=0
SUT1=1
BODEN=0
BODLEVEL=1
BOOTRST=1
BOOTSZ0=1
BOOTSZ1=1
EESAVE=1
CKOPT=0
SPIEN=0
JTAGEN=1
OCDEN=1
WDTON=1
S8515C=1
[Lock bits]
LockBit1=1
LockBit2=1
BootLockBit01=1
BootLockBit02=1
BootLockBit11=1
BootLockBit12=1
[TemplatesForm]
Opened=0
Left=198
Top=106
[EEMacroOptions]
WaitEEWEBefore=1
LockGlobalInterrupt=0
[SRAM]
External=0
[Programmer]
Counter=1
Check device=1
Chip erase=1
Write to program=1
Write to EEPROM=0
Write fuse bits=1
Write lock bits=0
Copy calibration byte=0
Close on completion=1
Calibration byte address=0
Calibration byte EEPROM address=0
[Program]
Fill value=0
[Chip reader]
Flash file name=
EEPROM file name=
[Compiler]
Auto declaring fragments of working registers=1
Optimization=1
Round immediate data=1
[Debug]
Configuration=0
[Port]
Deceleration=2
[Control]
Read only=0
[MainWindow]
Left=0
Top=0
Width=1280
Height=1024
