AY-Player

Version 7.1 (19.11.2014) Now it uses multimedia timer!

New serial protocol from version 6.0
- Baud Rate: 57600
- Data Bits: 8
- Stop Bits: 1
- Parity: NONE
- Registers are sent as 2 values 1) Register number 0-13, 2) Register value
- To synchronize, just send 0xFF at start sending

Used with emulator to play PSG,VTX,YM etc. on PC

AYPlayer_x86.exe 32 bit version
AYPlayer_x64.exe 64 bit version


ORIGIN: http://www.avray.ru